Wang, Y., Yang, L., Hu, R., Sun, W., Liu, J., Ouyang, L., . . . Zhu, M. (2015). A stable and high-capacity anode for lithium-ion battery: Fe2O3 wrapped by few layered graphene. JOURNAL OF POWER SOURCES, 288, 314-319. doi:10.1016/j.jpowsour.2015.04.076
Wei, Y., Xue, J., Fang, W., Chen, Y., Wang, H., & Caro, J. (2015). Enhanced stability of Zr-doped Ba(CeTb)O<inf>3-δ</inf>-Ni cermet membrane for hydrogen separation. Chemical Communications, 51(58), 11619-11621. doi:10.1039/c5cc03391h
Peng, J., Xian, S., Xiao, J., Huang, Y., Xia, Q., Wang, H., & Li, Z. (2015). A supported Cu(I)@MIL-100(Fe) adsorbent with high CO adsorption capacity and CO/N-2 selectivity. CHEMICAL ENGINEERING JOURNAL, 270, 282-289. doi:10.1016/j.cej.2015.01.126
Xian, S., Peng, J., Zhang, Z., Xia, Q., Wang, H., & Li, Z. (2015). Highly enhanced and weakened adsorption properties of two MOFs by water vapor for separation of CO2/CH4 and CO2/N-2 binary mixtures. CHEMICAL ENGINEERING JOURNAL, 270, 385-392. doi:10.1016/j.cej.2015.02.041
Chen, Y., Liao, Q., Li, Z., Wang, H., Wei, Y., Feldhoff, A., & Caro, J. (2015). A CO2-stable hollow-fiber membrane with high hydrogen permeation flux. AICHE JOURNAL, 61(6), 1997-2007. doi:10.1002/aic.14772
Guo, M., Wang, S., Ding, L. X., Huang, C., & Wang, H. (2015). Tantalum-doped lithium titanate with enhanced performance for lithium-ion batteries. Journal of Power Sources, 283, 372-380. doi:10.1016/j.jpowsour.2015.02.154
Li, Y., Li, Y., Chen, R., Sharafudeen, K., Zhou, S., Gecevicius, M., . . . Qiu, J. (2015). Tailoring of the trap distribution and crystal field in Cr3+-doped non-gallate phosphors with near-infrared long-persistence phosphorescence. NPG ASIA MATERIALS, 7(5), 11 pages. doi:10.1038/am.2015.38
Zhou, X., Huang, W., Miao, J., Xia, Q., Zhang, Z., Wang, H., & Li, Z. (2015). Enhanced separation performance of a novel composite material GrO@MIL-101 for CO2/CH4 binary mixture. CHEMICAL ENGINEERING JOURNAL, 266, 339-344. doi:10.1016/j.cej.2014.12.021
Xiao, K., Xia, L., Liu, G., Wang, S., Ding, L. X., & Wang, H. (2015). Honeycomb-like NiMoO4 ultrathin nanosheet arrays for high-performance electrochemical energy storage. Journal of Materials Chemistry A, 3(11), 6128-6135. doi:10.1039/c5ta00258c
Xian, S., Yu, Y., Xiao, J., Zhang, Z., Xia, Q., Wang, H., & Li, Z. (2015). Competitive adsorption of water vapor with VOCs dichloroethane, ethyl acetate and benzene on MIL-101(Cr) in humid atmosphere. RSC ADVANCES, 5(3), 1827-1834. doi:10.1039/c4ra10463c
Li, Z., Liu, G., Guo, M., Ding, L. X., Wang, S., & Wang, H. (2015). Electrospun porous vanadium pentoxide nanotubes as a high-performance cathode material for lithium-ion batteries. Electrochimica Acta, 173, 131-138. doi:10.1016/j.electacta.2015.05.057
Zhang, L., Wei, M., Wang, S., Li, Z., Ding, L. X., & Wang, H. (2015). Highly stable PtP alloy nanotube arrays as a catalyst for the oxygen reduction reaction in acidic medium. CHEMICAL SCIENCE, 6(5), 3211-3216. doi:10.1039/c5sc00124b
Wei, Y., Xue, J., Wang, H., & Caro, J. (2015). Hydrogen permeability and stability of BaCe(0.85)Tb(0.05)Zr(0.1)O(3-δ) asymmetric membranes. Journal of Membrane Science, 488, 173-181. doi:10.1016/j.memsci.2015.04.035
Guo, M., Wang, S., Ding, L. X., Zheng, L., & Wang, H. (2015). Synthesis of novel nitrogen-doped lithium titanate with ultra-high rate capability using melamine as a solid nitrogen source. Journal of Materials Chemistry A, 3(20), 10753-10759. doi:10.1039/c5ta01179e
Chen, S., Liu, G., Yadegari, H., Wang, H., & Qiao, S. Z. (2015). Three-dimensional MnO2 ultrathin nanosheet aerogels for high-performance Li-O-2 batteries. JOURNAL OF MATERIALS CHEMISTRY A, 3(6), 2559-2563. doi:10.1039/c5ta00004a
Sun, W., Hu, R., Liu, H., Zeng, M., Yang, L., Wang, H., & Zhu, M. (2014). Embedding nano-silicon in graphene nanosheets by plasma assisted milling for high capacity anode materials in lithium ion batteries. JOURNAL OF POWER SOURCES, 268, 610-618. doi:10.1016/j.jpowsour.2014.06.039
Cai, W., Wang, H., Liu, J., Jiao, L., Wang, Y., Ouyang, L., . . . Zhu, M. (2014). Towards easy reversible dehydrogenation of LiBH4 by catalyzing hierarchic nanostructured CoB. NANO ENERGY, 10, 235-244. doi:10.1016/j.nanoen.2014.09.001
Li, D., Ding, L. X., Chen, H., Wang, S., Li, Z., Zhu, M., & Wang, H. (2014). Novel nitrogen-rich porous carbon spheres as a high-performance anode material for lithium-ion batteries. JOURNAL OF MATERIALS CHEMISTRY A, 2(39), 16617-16622. doi:10.1039/c4ta03281k
Liao, Q., Wang, Y., Chen, Y., Wei, Y., & Wang, H. (2014). Novel bifunctional tantalum and bismuth co-doped perovskite BaBi0.05Co0.8Th0.15O3-delta with high oxygen permeation. JOURNAL OF MEMBRANE SCIENCE, 468, 184-191. doi:10.1016/j.memsci.2014.06.005
Wu, Y., Xiao, J., Wu, L., Chen, M., Xi, H., Li, Z., & Wang, H. (2014). Adsorptive Denitrogenation of Fuel over Metal Organic Frameworks: Effect of N-Types and Adsorption Mechanisms. JOURNAL OF PHYSICAL CHEMISTRY C, 118(39), 22533-22543. doi:10.1021/jp5045817
Wei, Y., Liao, Q., Li, Z., Wang, H., Feldhoff, A., & Caro, J. (2014). Partial Oxidation of Methane in Hollow-Fiber Membrane Reactors Based on Alkaline-Earth Metal-Free CO2-Tolerant Oxide. AICHE JOURNAL, 60(10), 3587-3595. doi:10.1002/aic.14540
Wu, J., Xia, Q., Wang, H., & Li, Z. (2014). Catalytic performance of plasma catalysis system with nickel oxide catalysts on different supports for toluene removal: Effect of water vapor. APPLIED CATALYSIS B-ENVIRONMENTAL, 156, 265-272. doi:10.1016/j.apcatb.2014.03.017
Cai, D., Ding, L., Wang, S., Li, Z., Zhu, M., & Wang, H. (2014). Facile synthesis of ultrathin-shell graphene hollow spheres for high-performance lithium-ion batteries. ELECTROCHIMICA ACTA, 139, 96-103. doi:10.1016/j.electacta.2014.07.014
Lian, P., Wang, J., Cai, D., Liu, G., Wang, Y., & Wang, H. (2014). Design and synthesis of porous nano-sized Sn@C/graphene electrode material with 3D carbon network for high-performance lithium-ion batteries. JOURNAL OF ALLOYS AND COMPOUNDS, 604, 188-195. doi:10.1016/j.jallcom.2014.03.116
Zhan, L., Wang, S., Ding, L. X., Li, Z., & Wang, H. (2014). Grass-like Co3O4 nanowire arrays anode with high rate capability and excellent cycling stability for lithium-ion batteries. ELECTROCHIMICA ACTA, 135, 35-41. doi:10.1016/j.electacta.2014.04.139
Huang, W., Zhou, X., Xia, Q., Peng, J., Wang, H., & Li, Z. (2014). Preparation and Adsorption Performance of GrO@Cu-BTC for Separation of CO2/CH4. INDUSTRIAL & ENGINEERING CHEMISTRY RESEARCH, 53(27), 11176-11184. doi:10.1021/ie501040s
Chen, J., Wang, S., Ding, L., Jiang, Y., & Wang, H. (2014). Performance of through-hole anodic aluminum oxide membrane as a separator for lithium-ion battery. JOURNAL OF MEMBRANE SCIENCE, 461, 22-27. doi:10.1016/j.memsci.2014.03.005
Cai, D., Wang, S., Ding, L., Lian, P., Zhang, S., Peng, F., & Wang, H. (2014). Superior cycle stability of graphene nanosheets prepared by freeze-drying process as anodes for lithium-ion batteries. JOURNAL OF POWER SOURCES, 254, 198-203. doi:10.1016/j.jpowsour.2013.12.136
Wang, Y., Liao, Q., Zhou, L., & Wang, H. (2014). Oxygen permeability and structure stability of a novel cobalt-free perovskite Gd0.33Ba0.67FeO3-delta. JOURNAL OF MEMBRANE SCIENCE, 457, 82-87. doi:10.1016/j.memsci.2014.01.046
Luo, J., Yu, H., Wang, H., Wang, H., & Peng, F. (2014). Aerobic oxidation of benzyl alcohol to benzaldehyde catalyzed by carbon nanotubes without any promoter. CHEMICAL ENGINEERING JOURNAL, 240, 434-442. doi:10.1016/j.cej.2013.11.093
Zhang, S., Zhang, S., Peng, B., Wang, H., Yu, H., Wang, H., & Peng, F. (2014). High performance hydrogenated TiO2 nanorod arrays as a photoelectrochemical sensor for organic compounds under visible light. ELECTROCHEMISTRY COMMUNICATIONS, 40, 24-27. doi:10.1016/j.elecom.2013.12.013
Wu, L., Xiao, J., Wu, Y., Xian, S., Miao, G., Wang, H., & Li, Z. (2014). A Combined Experimental/Computational Study on the Adsorption of Organosulfur Compounds over Metal-Organic Frameworks from Fuels. LANGMUIR, 30(4), 1080-1088. doi:10.1021/la404540j
Liao, Q., Chen, Y., Wei, Y., Zhou, L., & Wang, H. (2014). Performance of U-shaped BaCo0.7Fe0.2Ta0.1O3-delta hollow-fiber membranes reactor with high oxygen permeation for methane conversion. CHEMICAL ENGINEERING JOURNAL, 237, 146-152. doi:10.1016/j.cej.2013.09.105
Lian, P., Wang, J., Cai, D., Ding, L., Jia, Q., & Wang, H. (2014). Porous SnO2@C/graphene nanocomposite with 3D carbon conductive network as a superior anode material for lithium-ion batteries. ELECTROCHIMICA ACTA, 116, 103-110. doi:10.1016/j.electacta.2013.11.007
Luo, H., Klande, T., Cao, Z., Liang, F., Wang, H., & Caro, J. (2014). A CO2-stable reduction-tolerant Nd-containing dual phase membrane for oxyfuel CO2 capture. JOURNAL OF MATERIALS CHEMISTRY A, 2(21), 7780-7787. doi:10.1039/c3ta14870j
Zhou, X., Huang, W., Shi, J., Zhao, Z., Xia, Q., Li, Y., . . . Li, Z. (2014). A novel MOF/graphene oxide composite GrO@MIL-101 with high adsorption capacity for acetone. JOURNAL OF MATERIALS CHEMISTRY A, 2(13), 4722-4730. doi:10.1039/c3ta15086k
Chen, J., Wang, S., Cai, D., & Wang, H. (2014). Porous SiO2 as a separator to improve the electrochemical performance of spinel LiMn2O4 cathode. JOURNAL OF MEMBRANE SCIENCE, 449, 169-175. doi:10.1016/j.memsci.2013.08.028
Li, S., Wang, Y., Qiu, J., Ling, M., Wang, H., Martens, W., & Zhang, S. (2014). SnO2 decorated graphene nanocomposite anode materials prepared via an up-scalable wet-mechanochemical process for sodium ion batteries. RSC ADVANCES, 4(91), 50148-50152. doi:10.1039/c4ra09699a
Li, D., Ding, L. X., Wang, S., Cai, D., & Wang, H. (2014). Ultrathin and highly-ordered CoO nanosheet arrays for lithium-ion batteries with high cycle stability and rate capability. JOURNAL OF MATERIALS CHEMISTRY A, 2(16), 5625-5630. doi:10.1039/c3ta14826b
Zheng, Q., Xue, J., Liao, Q., Wei, Y., Li, Z., & Wang, H. (2013). CO2-tolerant alkaline-earth metal-free single phase membrane for oxygen separation. CHEMICAL ENGINEERING SCIENCE, 101, 240-247. doi:10.1016/j.ces.2013.06.039
Xue, J., Liao, Q., Wei, Y., Li, Z., & Wang, H. (2013). A CO2-tolerance oxygen permeable 60Ce(0.9)Gd(0.1)O(2-delta)-40Ba(0.5)Sr(0.5)Co(0.8)Fe(0.2)O(3-delta) dual phase membrane. JOURNAL OF MEMBRANE SCIENCE, 443, 124-130. doi:10.1016/j.memsci.2013.04.067
Yu, L., Cai, D., Wang, H., & Titirici, M. M. (2013). Synthesis of Microspherical LiFePO4-Carbon Composites for Lithium-Ion Batteries. NANOMATERIALS, 3(3), 443-452. doi:10.3390/nano3030443
Peng, S., Wei, Y., Xue, J., Chen, Y., & Wang, H. (2013). Pr1.8La0.2Ni0.74Cu0.21Ga0.05O4+delta as a potential cathode material with CO2 resistance for intermediate temperature solid oxide fuel cell. INTERNATIONAL JOURNAL OF HYDROGEN ENERGY, 38(25), 10552-10558. doi:10.1016/j.ijhydene.2013.06.073
Lian, P., Cai, D., Luo, K., Jia, Y., Sun, Y., & Wang, H. (2013). Preparation and electrochemical properties of (Fe2.5Ti0.5)(1.04)O-4-graphene nanocomposite. ELECTROCHIMICA ACTA, 104, 267-273. doi:10.1016/j.electacta.2013.04.130
Chen, Y., Liao, Q., Wei, Y., Li, Z., & Wang, H. (2013). A CO2-Stable K2NiF4-Type Oxide (Nd0.9La0.1)(2)(Ni0.74Cu0.21Al0.05)O4+delta for Oxygen Separation. INDUSTRIAL & ENGINEERING CHEMISTRY RESEARCH, 52(25), 8571-8578. doi:10.1021/ie4008369
Zhang, Z., Xian, S., Xia, Q., Wang, H., Li, Z., & Li, J. (2013). Enhancement of CO2 Adsorption and CO2/N2 Selectivity on ZIF-8 via Postsynthetic Modification. AICHE JOURNAL, 59(6), 2195-2206. doi:10.1002/aic.13970
Wei, Y., Yang, W., Caro, J., & Wang, H. (2013). Dense ceramic oxygen permeable membranes and catalytic membrane reactors. CHEMICAL ENGINEERING JOURNAL, 220, 185-203. doi:10.1016/j.cej.2013.01.048
Zhang, L., Wang, S., Cai, D., Lian, P., Zhu, X., Yang, W., & Wang, H. (2013). Li3V2(PO4)(3)@C/graphene composite with improved cycling performance as cathode material for lithium-ion batteries. ELECTROCHIMICA ACTA, 91, 108-113. doi:10.1016/j.electacta.2012.12.098
Wei, Y., Ravkina, O., Klande, T., Wang, H., & Feldhoff, A. (2013). Effect of CO2 and SO2 on oxygen permeation and microstructure of (Pr0.9La0.1)(2)(Ni0.74Cu0.21Ga0.05)O4+delta membranes. JOURNAL OF MEMBRANE SCIENCE, 429, 147-154. doi:10.1016/j.memsci.2012.11.075
Cai, D., Wang, S., Lian, P., Zhu, X., Li, D., Yang, W., & Wang, H. (2013). Superhigh capacity and rate capability of high-level nitrogen-doped graphene sheets as anode materials for lithium-ion batteries. ELECTROCHIMICA ACTA, 90, 492-497. doi:10.1016/j.electacta.2012.11.105
Wei, Y., Liao, Q., Xue, J., Li, Z., & Wang, H. (2013). Influence of SO2 on the phase structure, oxygen permeation and microstructure of K2NiE4-type hollow fiber membranes. CHEMICAL ENGINEERING JOURNAL, 217, 34-40. doi:10.1016/j.cej.2012.12.009
Wei, Y., Liao, Q., Li, Z., & Wang, H. (2013). Enhancement of oxygen permeation through U-shaped K₂NiF₄-type oxide hollow fiber membranes by surface modifications. Separation and Purification Technology, 110, 74-80. doi:10.1016/j.seppur.2013.03.006
Zhang, P., Qiu, J., Zheng, Z., Liu, G., Ling, M., Martens, W., . . . Zhang, S. (2013). Free-standing and bendable carbon nanotubes/TiO₂ nanofibres composite electrodes for flexible lithium ion batteries. Electrochimica Acta, 104, 41-47. doi:10.1016/j.electacta.2013.04.089
Cai, D., Li, D., Wang, S., Zhu, X., Yang, W., Zhang, S., & Wang, H. (2013). High rate capability of TiO₂/nitrogen-doped graphene nanocomposite as an anode material for lithium-ion batteries. Journal of Alloys and Compounds, 561, 54-58. doi:10.1016/j.jallcom.2013.01.068
Yu, L., Cai, D., Wang, H., & Titirici, M. M. (2013). Hydrothermal synthesis of SnO2 and SnO2@C nanorods and their application as anode materials in lithium-ion batteries. RSC ADVANCES, 3(38), 17281-17286. doi:10.1039/c3ra42900h
Wei, Y., Wang, Y., Tang, J., Li, Z., & Wang, H. (2013). Oxy-fuel combustion for CO₂ capture using a CO₂-tolerant oxygen transporting membrane. AIChE Journal, 59(10), 3856-3862. doi:10.1002/aic.14131
Luo, H., Jiang, H., Klande, T., Liang, F., Cao, Z., Wang, H., & Caro, J. (2012). Rapid glycine-nitrate combustion synthesis of the CO2-stable dual phase membrane 40Mn(1.5)Co(1.5)O(4-delta)-60Ce(0.9)Pr(0.1)O(2-delta) for CO2 capture via an oxy-fuel process. JOURNAL OF MEMBRANE SCIENCE, 423, 450-458. doi:10.1016/j.memsci.2012.08.046
Liao, Q., Zheng, Q., Xue, J., Wei, Y., & Wang, H. (2012). U-Shaped BaCo0.7Fe0.2Ta0.1O3-delta Hollow-Fiber Membranes with High Permeation for Oxygen Separation. INDUSTRIAL & ENGINEERING CHEMISTRY RESEARCH, 51(46), 15217-15223. doi:10.1021/ie301789t
Peng, S., Zhou, D., Wei, Y., Li, Z., & Wang, H. (2012). A novel U-shaped anode-supported hollow fiber solid oxide fuel cell with considerable thermal cycling performance and stability. JOURNAL OF MEMBRANE SCIENCE, 417, 80-86. doi:10.1016/j.memsci.2012.06.016
Wei, Y., Tang, J., Zhou, L., Xue, J., Li, Z., & Wang, H. (2012). Oxygen separation through U-shaped hollow fiber membrane using pure CO2 as sweep gas. AICHE JOURNAL, 58(9), 2856-2864. doi:10.1002/aic.12802
Cai, D., Lian, P., Zhu, X., Liang, S., Yang, W., & Wang, H. (2012). High specific capacity of TiO2-graphene nanocomposite as an anode material for lithium-ion batteries in an enlarged potential window. ELECTROCHIMICA ACTA, 74, 65-72. doi:10.1016/j.electacta.2012.03.170
Chen, J., Xiang, H., Zhang, L., & Wang, H. (2012). Self-standing integrative cell with an inorganic separator for lithium-ion battery stacks. JOURNAL OF APPLIED ELECTROCHEMISTRY, 42(7), 471-475. doi:10.1007/s10800-012-0421-5
Xiao, F., Chen, R., Shen, Y. Q., Dong, Z. L., Wang, H. H., Zhang, Q. Y., & Sun, H. D. (2012). Efficient energy transfer and enhanced infrared emission in Er-oped ZnO-SiO 2 omposites. Journal of Physical Chemistry C, 116(24), 13458-13462. doi:10.1021/jp304075g
Luo, H., Jiang, H., Klande, T., Cao, Z., Liang, F., Wang, H., & Caro, J. (2012). Novel Cobalt-Free, Noble Metal-Free Oxygen-Permeable 40Pr(0.6)Sr(0.4)FeO(3-delta)-60Ce(0.9)Pr(0.1)O(2-delta), Dual-Phase Membrane. CHEMISTRY OF MATERIALS, 24(11), 2148-2154. doi:10.1021/cm300710p
Zhou, D., Peng, S., Wei, Y., Li, Z., & Wang, H. (2012). Novel asymmetric anode-supported hollow fiber solid oxide fuel cell. JOURNAL OF ALLOYS AND COMPOUNDS, 523, 134-138. doi:10.1016/j.jallcom.2012.01.120
Zhang, L., Xiang, H., Li, Z., & Wang, H. (2012). Porous Li3V2(PO4)(3)/C cathode with extremely high-rate capacity prepared by a sot-gel-combustion method for fast charging and discharging. JOURNAL OF POWER SOURCES, 203, 121-125. doi:10.1016/j.jpowsour.2011.11.082
Xue, J., Zheng, Q., Wei, Y., Yuan, K., Li, Z., & Wang, H. (2012). Dual Phase Composite Oxide of Ce0.9Gd0.1O2-delta-Ba0.5Sr0.5Co0.8Fe0.2O3-delta with Excellent Oxygen Permeation. INDUSTRIAL & ENGINEERING CHEMISTRY RESEARCH, 51(12), 4703-4709. doi:10.1021/ie300083r
Wei, Y. Y., Zhou, L. Y., Tang, J., Li, Z., & Wang, H. H. (2012). Activation in the initial stage of oxygen permeation in SrCo₀.₉Ta₀.₁O₃–δ. Chinese Chemical Letters, 23(1), 113-116. doi:10.1016/j.cclet.2011.09.020
Tian, B., Xiang, H., Zhang, L., & Wang, H. (2012). Effect of Nb-doping on electrochemical stability of Li4Ti5O12 discharged to 0 V. JOURNAL OF SOLID STATE ELECTROCHEMISTRY, 16(1), 205-211. doi:10.1007/s10008-011-1305-z
Xiang, H. F., Li, Z. D., Xie, K., Jiang, J. Z., Chen, J. J., Lian, P. C., . . . Wang, H. H. (2012). Graphene sheets as anode materials for Li-ion batteries: preparation, structure, electrochemical properties and mechanism for lithium storage. RSC Advances, 2(17), 6792-6799. doi:10.1039/c2ra20549a
Wei, Y., Tang, J., Zhou, L., Li, Z., & Wang, H. (2012). One end-dead perovskite hollow fiber membranes for high-purity oxygen production from ambient air. Chemical Engineering Journal, 183, 473-482. doi:10.1016/j.cej.2011.12.038
Tang, J., Wei, Y., Zhou, L., Li, Z., & Wang, H. (2012). Oxygen permeation through a CO₂-tolerant mixed conducting oxide (Pr₀.₉La₀.₁)₂(Ni₀.₇₄Cu₀.₂₁Ga₀.₀₅)O₄₊δ. AIChE Journal, 58(8), 2473-2478. doi:10.1002/aic.12742
Zhang, L., Xiang, H., Zhu, X., Yang, W., & Wang, H. (2012). Synthesis of LiFePO₄/C composite as a cathode material for lithium-ion battery by a novel two-step method. Journal of Materials Science, 47(7), 3076-3081. doi:10.1007/s10853-011-6139-7
Lian, P., Liang, S., Zhu, X., Yang, W., & Wang, H. (2011). A novel Fe3O4-SnO2-graphene ternary nanocomposite as an anode material for lithium-ion batteries. ELECTROCHIMICA ACTA, 58, 81-88. doi:10.1016/j.electacta.2011.08.088
Luo, H., Jiang, H., Efimov, K., Liang, F., Wang, H., & Caro, J. (2011). CO2-Tolerant Oxygen-Permeable Fe2O3-Ce0.9Gd0.1O2-delta Dual Phase Membranes. INDUSTRIAL & ENGINEERING CHEMISTRY RESEARCH, 50(23), 13508-13517. doi:10.1021/ie200517t
Wei, Y. Y., Huang, L., Tang, J., Zhou, L. Y., Li, Z., & Wang, H. H. (2011). Syngas production in a novel perovskite membrane reactor with co-feed of CO2
. Chinese Chemical Letters, 22(12), 1492-1496. doi:10.1016/j.cclet.2011.05.040
Wei, Y., Tang, J., Zhou, L., Li, Z., & Wang, H. (2011). Oxygen Permeation through U-Shaped K2NiF4-Type Oxide Hollow-Fiber Membranes. INDUSTRIAL & ENGINEERING CHEMISTRY RESEARCH, 50(22), 12727-12734. doi:10.1021/ie201298x
Xiang, H., Chen, J., Li, Z., & Wang, H. (2011). An inorganic membrane as a separator for lithium-ion battery. JOURNAL OF POWER SOURCES, 196(20), 8651-8655. doi:10.1016/j.jpowsour.2011.06.055
Zhang, Z., Xian, S., Xi, H., Wang, H., & Li, Z. (2011). Improvement of CO2 adsorption on ZIF-8 crystals modified by enhancing basicity of surface. CHEMICAL ENGINEERING SCIENCE, 66(20), 4878-4888. doi:10.1016/j.ces.2011.06.051
Luo, H., Jiang, H., Efimov, K., Caro, J., & Wang, H. (2011). Influence of the Preparation Methods on the Microstructure and Oxygen Permeability of a CO2-Stable Dual Phase Membrane. AICHE JOURNAL, 57(10), 2738-2745. doi:10.1002/aic.12488
Liu, H., Wei, Y., Huang, L., & Wang, H. (2011). CHLORINE-DOPED Ba0.5Sr0.5Co0.8Fe0.2O3-delta AS AN OXYGEN-PERMEABLE MEMBRANE AT INTERMEDIATE TEMPERATURE. FUNCTIONAL MATERIALS LETTERS, 4(3), 261-264. doi:10.1142/S1793604711001932
Xiang, H. F., Wang, Q., Wang, D. Z., Zhang, D. W., Wang, H. H., & Chen, C. H. (2011). Optimizing the compatibility between dimethyl methylphosphonate (DMMP)-based electrolytes and carbonaceous anodes. Journal of Applied Electrochemistry, 41(8), 965-971. doi:10.1007/s10800-011-0323-y
Xiang, H., Zhang, D., Jin, Y., Chen, C., Wu, J., & Wang, H. (2011). Hydrothermal synthesis of ultra-thin LiFePO4 platelets for Li-ion batteries. JOURNAL OF MATERIALS SCIENCE, 46(14), 4906-4912. doi:10.1007/s10853-011-5403-1
Xiang, H., Tian, B., Lian, P., Li, Z., & Wang, H. (2011). Sol-gel synthesis and electrochemical performance of Li4Ti5O12/graphene composite anode for lithium-ion batteries. JOURNAL OF ALLOYS AND COMPOUNDS, 509(26), 7205-7209. doi:10.1016/j.jallcom.2011.04.065
Xiang, H., Chen, J., & Wang, H. (2011). Effect of vinyl ethylene carbonate on the compatibility between graphite and the flame-retarded electrolytes containing dimethyl methyl phosphonate. IONICS, 17(5), 415-420. doi:10.1007/s11581-011-0527-5
Xiang, H. F., Shi, J. Y., Feng, X. Y., Ge, X. W., Wang, H. H., & Chen, C. H. (2011). Graphitic platelets prepared by electrochemical exfoliation of graphite and their application for Li energy storage. Electrochimica Acta, 56(15), 5322-5327. doi:10.1016/j.electacta.2011.04.001
Liang, S., Zhu, X., Lian, P., Yang, W., & Wang, H. (2011). Superior cycle performance of Sn@C/graphene nanocomposite as an anode material for lithium-ion batteries. JOURNAL OF SOLID STATE CHEMISTRY, 184(6), 1400-1404. doi:10.1016/j.jssc.2011.03.052
Lian, P., Zhu, X., Liang, S., Li, Z., Yang, W., & Wang, H. (2011). High reversible capacity of SnO2/graphene nanocomposite as an anode material for lithium-ion batteries. ELECTROCHIMICA ACTA, 56(12), 4532-4539. doi:10.1016/j.electacta.2011.01.126
Wei, Y., Liu, H., Xue, J., Li, Z., & Wang, H. (2011). Preparation and Oxygen Permeation of U-Shaped Perovskite Hollow-Fiber Membranes. AICHE JOURNAL, 57(4), 975-984. doi:10.1002/aic.12321
Chen, X., Huang, L., Wei, Y., & Wang, H. (2011). Tantalum stabilized SrCoO3-delta perovskite membrane for oxygen separation. JOURNAL OF MEMBRANE SCIENCE, 368(1-2), 159-164. doi:10.1016/j.memsci.2010.11.040
Luo, H., Efimov, K., Jiang, H., Feldhoff, A., Wang, H., & Caro, J. (2011). CO2-Stable and Cobalt-Free Dual-Phase Membrane for Oxygen Separation. ANGEWANDTE CHEMIE-INTERNATIONAL EDITION, 50(3), 759-763. doi:10.1002/anie.201003723
Lian, P., Zhu, X., Xiang, H., Li, Z., Yang, W., & Wang, H. (2010). Enhanced cycling performance of Fe3O4-graphene nanocomposite as an anode material for lithium-ion batteries. ELECTROCHIMICA ACTA, 56(2), 834-840. doi:10.1016/j.electacta.2010.09.086
Liu, H., Wei, Y., Caro, J., & Wang, H. (2010). Oxidative Coupling of Methane with High C-2 Yield by using Chlorinated Perovskite Ba0.5Sr0.5Fe0.2Co0.8O3-delta as Catalyst and N2O as Oxidant. CHEMCATCHEM, 2(12), 1539-1542. doi:10.1002/cctc.201000217
Jiang, H., Wang, H., Liang, F., Werth, S., Schirrmeister, S., Schiestel, T., & Caro, J. (2010). Improved water dissociation and nitrous oxide decomposition by in situ oxygen removal in perovskite catalytic membrane reactor. CATALYSIS TODAY, 156(3-4), 187-190. doi:10.1016/j.cattod.2010.02.027
Tian, B., Xiang, H., Zhang, L., Li, Z., & Wang, H. (2010). Niobium doped lithium titanate as a high rate anode material for Li-ion batteries. ELECTROCHIMICA ACTA, 55(19), 5453-5458. doi:10.1016/j.electacta.2010.04.068
Zhang, Z., Xu, M., Wang, H., & Li, Z. (2010). Enhancement of CO2 adsorption on high surface area activated carbon modified by N-2, H-2 and ammonia. CHEMICAL ENGINEERING JOURNAL, 160(2), 571-577. doi:10.1016/j.cej.2010.03.070
Lian, P., Zhu, X., Liang, S., Li, Z., Yang, W., & Wang, H. (2010). Large reversible capacity of high quality graphene sheets as an anode material for lithium-ion batteries. ELECTROCHIMICA ACTA, 55(12), 3909-3914. doi:10.1016/j.electacta.2010.02.025
Luo, H., Wei, Y., Jiang, H., Yuan, W., Lv, Y., Caro, J., & Wang, H. (2010). Performance of a ceramic membrane reactor with high oxygen flux Ta-containing perovskite for the partial oxidation of methane to syngas. JOURNAL OF MEMBRANE SCIENCE, 350(1-2), 154-160. doi:10.1016/j.memsci.2009.12.023
Luo, H., Tian, B., Wei, Y., Wang, H., Jiang, H., & Caro, J. (2010). Oxygen Permeability and Structural Stability of a Novel Tantalum-Doped Perovskite BaCo0.7Fe0.2Ta0.1O3-delta. AICHE JOURNAL, 56(3), 604-610. doi:10.1002/aic.12044
Jiang, H., Liang, F., Czuprat, O., Efimov, K., Feldhoff, A., Schirrmeister, S., . . . Caro, J. (2010). Hydrogen Production by Water Dissociation in Surface-Modified BaCoxFeyZr1-x-yO3-delta Hollow-Fiber Membrane Reactor with Improved Oxygen Permeation. CHEMISTRY-A EUROPEAN JOURNAL, 16(26), 7898-7903. doi:10.1002/chem.200902494
Yu, L., Liu, Q., & Wang, H. (2009). Synthesis of LiFePO4-C cathode materials using a green and low-cost method. IONICS, 15(6), 689-692. doi:10.1007/s11581-009-0389-2
Liu, Q., Yu, L., & Wang, H. (2009). Preparation of LiMn2O4 with an enhanced performance by mixed liquid and mechanical activations. JOURNAL OF ALLOYS AND COMPOUNDS, 486(1-2), 886-889. doi:10.1016/j.jallcom.2009.07.087
Cai, M., Liu, S., Efimov, K., Caro, J., Feldhoff, A., & Wang, H. (2009). Preparation and hydrogen permeation of BaCe0.95Nd0.05O3-delta membranes. JOURNAL OF MEMBRANE SCIENCE, 343(1-2), 90-96. doi:10.1016/j.memsci.2009.07.011
Wang, H., Feldhoff, A., Caro, J., Schiestel, T., & Werth, S. (2009). Oxygen Selective Ceramic Hollow Fiber Membranes for Partial Oxidation of Methane. AICHE JOURNAL, 55(10), 2657-2664. doi:10.1002/aic.11856
Chen, X., Liu, H., Wei, Y., Caro, J., & Wang, H. (2009). A novel zincum-doped perovskite-type ceramic membrane for oxygen separation. JOURNAL OF ALLOYS AND COMPOUNDS, 484(1-2), 386-389. doi:10.1016/j.jallcom.2009.04.107
Luo, H. X., Yu, L. H., Chen, X. Z., Wang, H. H., & Caro, J. (2009). Novel Ba0.5Sr0.5Fe0.8Zn0.2O3-δ membranes for POM. Chinese Chemical Letters, 20(2), 250-252. doi:10.1016/j.cclet.2008.10.011
Kondratenko, E. V., Wang, H., Kondratenko, V. A., & Caro, J. (2009). Selective oxidation of CH4 and C2H6 over a mixed oxygen ion and electron conducting perovskite-A TAP and membrane reactors study. JOURNAL OF MOLECULAR CATALYSIS A-CHEMICAL, 297(2), 142-149. doi:10.1016/j.molcata.2008.09.015
Jiang, H., Wang, H., Liang, F., Werth, S., Schiestel, T., & Caro, J. (2009). Direct Decomposition of Nitrous Oxide to Nitrogen by In Situ Oxygen Removal with a Perovskite Membrane. ANGEWANDTE CHEMIE-INTERNATIONAL EDITION, 48(16), 2983-2986. doi:10.1002/anie.200804582
Jiang, H., Xing, L., Czuprat, O., Wang, H., Schirrmeister, S., Schiestel, T., & Caro, J. (2009). Highly effective NO decomposition by in situ removal of inhibitor oxygen using an oxygen transporting membrane. CHEMICAL COMMUNICATIONS, (44), 6738-6740. doi:10.1039/b912269a
Chen, X. Z., Yu, L. H., Liu, Q. S., Wang, H. H., & Li, Z. (2008). Preparation and application of perovskite hollow fiber oxygen permeable membrane. Wuji Cailiao Xuebao/Journal of Inorganic Materials, 23(6), 1216-1220. doi:10.3724/SP.J.1077.2008.01216
Cai, M. Y., Luo, H. X., Li, Z., Feldhoff, A., Caro, J., & Wang, H. H. (2008). Preparation and hydrogen permeation properties of BaCe0.95Nd0.05O3-δ membranes. Chinese Chemical Letters, 19(10), 1256-1259. doi:10.1016/j.cclet.2008.06.054
Wang, H., Tablet, C., & Caro, J. (2008). Oxygen production at low temperature using dense perovskite hollow fiber membranes. JOURNAL OF MEMBRANE SCIENCE, 322(1), 214-217. doi:10.1016/j.memsci.2008.05.038
Feldhoff, A., Arnold, M., Martynczuk, J., Gesing, T. M., & Wang, H. (2008). The sol-gel synthesis of perovskites by an EDTA/citrate complexing method involves nanoscale solid state reactions. Solid State Sciences, 10(6), 689-701. doi:10.1016/j.solidstatesciences.2007.11.030
Arnold, M., Martynczuk, J., Efimov, K., Wang, H., & Feldhoff, A. (2008). Grain boundaries as barrier for oxygen transport in perovskite-type membranes. JOURNAL OF MEMBRANE SCIENCE, 316(1-2), 137-144. doi:10.1016/j.memsci.2007.10.002
Zhu, X., Wang, H., & Yang, W. (2008). Relationship between homogeneity and oxygen permeability of composite membranes. JOURNAL OF MEMBRANE SCIENCE, 309(1-2), 120-127. doi:10.1016/j.memsci.2007.10.01
Jiang, H., Wang, H., Werth, S., Schiestel, T., & Caro, J. (2008). Simultaneous Production of Hydrogen and Synthesis Gas by Combining Water Splitting with Partial Oxidation of Methane in a Hollow-Fiber Membrane Reactor. ANGEWANDTE CHEMIE-INTERNATIONAL EDITION, 47(48), 9341-9344. doi:10.1002/anie.200803899
Arnold, M., Wang, H., Martynczuk, J., & Feldhoff, A. (2007). In situ study of the reaction sequence in the sol-gel synthesis of a (Ba0.5Sr0.5)(Co0.8Fe0.2)O3-delta perovskite by x-ray diffraction and transmission electron microscopy. JOURNAL OF THE AMERICAN CERAMIC SOCIETY, 90(11), 3651-3655. doi:10.1111/j.1551-2916.2007.01932.x
Martynczuk, J., Arnold, M., Wang, H., Caro, J., & Feldhoff, A. (2007). How (Ba0.5Sr0.5)(Fe0.8Zn0.2)O3-delta and (Ba0.5Sr0.5)(Co0.8Fe0.2)O3-delta perovskites form via an EDTA/citric acid complexing method. ADVANCED MATERIALS, 19(16), 2134-+. doi:10.1002/adma.200700322
Caro, J., Caspary, K. J., Hamel, C., Hoting, B., Koelsch, P., Langanke, B., . . . Werth, S. (2007). Perowskit hollow fibre membranes for the catalytic partial oxidation of methane to synthesis gas. CHEMIE INGENIEUR TECHNIK, 79(6), 831-842. doi:10.1002/cite.200700046
Arnold, M., Wang, H., & Feldhoff, A. (2007). Influence of CO2 on the oxygen permeation performance and the microstructure of perovskite-type (Ba0.5Sr0.5)(Co0.8Fe0.2)O3-delta membranes. JOURNAL OF MEMBRANE SCIENCE, 293(1-2), 44-52. doi:10.1016/j.memsci.2007.01.032
Zhu, X., Wang, H., & Yang, W. (2006). Structural stability and oxygen permeability of cerium lightly doped BaFeO3-delta ceramic membranes. SOLID STATE IONICS, 177(33-34), 2917-2921. doi:10.1016/j.ssi.2006.08.027
Wang, H., Tablet, C., Schiestel, T., Werth, S., & Caro, J. (2006). Partial oxidation of methane to syngas in a perovskite hollow fiber membrane reactor. CATALYSIS COMMUNICATIONS, 7(11), 907-912. doi:10.1016/j.catcom.2006.03.023
Zhu, X., Wang, H., Cong, Y., & Yang, W. (2006). Partial oxidation of methane to syngas in BaCe0.15Fe0.85O3-delta membrane reactors. CATALYSIS LETTERS, 111(3-4), 179-185. doi:10.1007/s10562-006-0145-4
Wang, H., Kölsch, P., Schiestel, T., Tablet, C., Werth, S., & Caro, J. (2006). Production of high-purity oxygen by perovskite hollow fiber membranes swept with steam. Journal of Membrane Science, 284(1-2), 5-8. doi:10.1016/j.memsci.2006.07.043
WANG, H., SCHIESTEL, T., TABLET, C., SCHROEDER, M., & CARO, J. (2006). Mixed oxygen ion and electron conducting hollow fiber membranes for oxygen separation. Solid State Ionics, 177(26-32), 2255-2259. doi:10.1016/j.ssi.2006.05.039
Hamel, C., Seidel-Morgenstern, A., Schiestel, T., Werth, S., Wang, H., Tablet, C., & Caro, J. (2006). Experimental and modeling study of the O2-enrichment by perovskite fibers. AIChE Journal, 52(9), 3118-3125. doi:10.1002/aic.10934
Wang, H., Tablet, C., Yang, W., & Caro, J. (2005). In situ high temperature X-ray diffraction studies of mixed ionic and electronic conducting perovskite-type membranes. Materials Letters, 59(28), 3750-3755. doi:10.1016/j.matlet.2005.06.067
Wang, H. H., Tablet, C., Feldhoff, A., & Caro, H. (2005). Investigation of phase structure, sintering, and permeability of perovskite-type Ba0.5Sr0.5Co0.8Fe0.2O3-delta membranes. JOURNAL OF MEMBRANE SCIENCE, 262(1-2), 20-26. doi:10.1016/j.memsci.2005.03.046
SCHIESTEL, T., KILGUS, M., PETER, S., CASPARY, K., WANG, H., & CARO, J. (2005). Hollow fibre perovskite membranes for oxygen separation. Journal of Membrane Science, 258(1-2), 1-4. doi:10.1016/j.memsci.2005.03.035
Wang, H., Tablet, C., Feldhoff, A., & Caro, J. (2005). A cobalt-free oxygen-permeable membrane based on the perovskite-type oxide Ba0.5Sr0.5Zn0.2Fe0.8O 3-δ
. Advanced Materials, 17(14), 1785-1788. doi:10.1002/adma.200401608
Yang, W. S., Wang, H. H., Zhu, X. F., & Lin, L. W. (2005). Development and application of oxygen permeable membrane in selective oxidation of light alkanes. TOPICS IN CATALYSIS, 35(1-2), 155-167. doi:10.1007/s11244-005-3820-6
Wang, H., Werth, S., Schiestel, T., & Caro, J. (2005). Perovskite hollow-fiber membranes for the production of oxygen-enriched air. Angewandte Chemie - International Edition, 44(42), 6906-6909. doi:10.1002/anie.200501914
Wang, H. H., Wang, R., Liang, D. T., & Yang, W. S. (2004). Experimental and modeling studies on Ba0.5Sr0.5Co0.8Fe0.2O3-delta (BSCF) tubular membranes for air separation. JOURNAL OF MEMBRANE SCIENCE, 243(1-2), 405-415. doi:10.1016/j.memsci.2004.07.003
Zhu, X. F., Wang, H. H., & Yang, W. S. (2004). Novel cobalt-free oxygen permeable membrane. CHEMICAL COMMUNICATIONS, (9), 1130-1131. doi:10.1039/b400857j
Wang, H. H., Yang, W. S., Cong, Y., Zhu, X. F., & Lin, Y. S. (2003). Structure and oxygen permeability of a dual-phase membrane. JOURNAL OF MEMBRANE SCIENCE, 224(1-2), 107-115. doi:10.1016/j.memsci.2003.07.003
Wang, H. H., Cong, Y., Yang, W. S., & Lin, L. W. (2003). Study on oxidative coupling of methane in oxygen permeable tubular membrane reactor. CHINESE JOURNAL OF CATALYSIS, 24(3), 169-174. Retrieved from http://gateway.webofknowledge.com/gateway/Gateway.cgi?GWVersion=2&SrcApp=PARTNER_APP&SrcAuth=LinksAMR&KeyUT=WOS:000182347400004&DestLinkType=FullRecord&DestApp=ALL_WOS&UsrCustomerID=1f051b2c0ced71d786748f61000f9895
Wang, H. H., Cong, Y., Zhu, X. F., & Yang, W. S. (2003). Oxidative dehydrogenation of propane in a dense tubular membrane reactor. REACTION KINETICS AND CATALYSIS LETTERS, 79(2), 351-356. doi:10.1023/A:1024502705982
Wang, H. H., Cong, Y., & Yang, W. S. (2002). Oxygen permeation study in a tubular Ba0.5Sr0.5Co0.8Fe0.2O3-delta oxygen permeable membrane. JOURNAL OF MEMBRANE SCIENCE, 210(2), 259-271. doi:10.1016/S0376-7388(02)00361-7
Wang, H. H., Cong, Y., & Yang, W. S. (2002). Continuous oxygen ion transfer medium as a catalyst for high selective oxidative dehydrogenation of ethane. CATALYSIS LETTERS, 84(1-2), 101-106. doi:10.1023/A:1021088904379
Wang, H. H., Cong, Y., & Yang, W. S. (2002). Partial oxidation of ethane to syngas in an oxygen-permeable membrane reactor. JOURNAL OF MEMBRANE SCIENCE, 209(1), 143-152. doi:10.1016/S0376-7388(02)00323-X
Wang, H. H., Cong, Y., & Yang, W. S. (2002). Partial oxidation of methane to syngas in tubular oxygen-permeable reactor. CHINESE SCIENCE BULLETIN, 47(7), 534-537. doi:10.1360/02tb9123
Wang, H. H., Cong, Y., & Yang, W. S. (2002). High selectivity of oxidative dehydrogenation of ethane to ethylene in an oxygen permeable membrane reactor. CHEMICAL COMMUNICATIONS, (14), 1468-1469. doi:10.1039/b203168j
Yang, W. S., Shao, Z. P., Cong, Y., Yang, P., & Wang, H. H. (2001). Synthesis, characterization and application of Ba0.5Sr0.5Co0.8Fe0.2O3-x oxygen permeable membrane.. ABSTRACTS OF PAPERS OF THE AMERICAN CHEMICAL SOCIETY, 221, U227. Retrieved from http://gateway.webofknowledge.com/gateway/Gateway.cgi?GWVersion=2&SrcApp=PARTNER_APP&SrcAuth=LinksAMR&KeyUT=WOS:000168824801327&DestLinkType=FullRecord&DestApp=ALL_WOS&UsrCustomerID=1f051b2c0ced71d786748f61000f9895